Note: Please send data as in below listed sheet or any other forms to our email: info@fountom.com

|  |  |  |  |
| --- | --- | --- | --- |
|  Client Name | *Fountom Marine* |  Destination Country | *China* |
|  Contact Email | *info@fountom.com* |  Delivery Terms | *FOB Shanghai* |
| **No.** | **Product Name** | **Nominal Size** | **Specification/Type** | **Material** | **Press.Rating** | **QTY** |
|
| Valves and Armatures |
| 1 | Air Vent | DN100 | (With flame arrestor) |  | PN10 | 1 |
| 2 | SDNR Valve | DN50 | Flanged Type | CI | PN10 | 3 |
| 3 | Buttterfly Valve | DN200 | Flanged Type | CI | PN10 | 2 |
| 4 | Globe Valve | DN32 | Flanged Type | CI | PN10 | 12 |
| 5 | Non Return Valve | DN25 | Flanged, Thread type | CI | PN10 | 1 |
| 6 | Strainer | DN65 | Mesh Size 5mm, flanged Type | CI | PN10 | 1 |
| 7 | Mud box | DN65 | Flanged Type | CI | PN10 | 3 |
| 8 | Fire Hydrant | DN50 | Flanged,angle Type | Brass | PN10 | 5 |
| 9 | Bilge Ejector | DN50/50/80 | 20m3/h@30MWC | CI | PN10 | 1 |
| 10 | Quick closing Valve | DN40 |  Flanged,Mechanical Type | Ductile Cast Iron | PN10 | 1 |
| 11 | Check Valve | DN32 | Swing check Type | CI | PN10 | 1 |
| 12 | Simplex Filter | DN50 | Mesh Size 300 micron ,flanged Type | CI | PN10 | 1 |
| 13 | Gate Valve | DN100 | Flanged Type | CI | PN10 | 3 |
| 14 | Self closing Drain Valve | DN20 | Flanged Type | CI | PN10 | 5 |
| 15 | Safety Relief Valve | DN100 | Flanged Type | CI | PN10 | 2 |
| 16 | Duplex LO Filter | DN100 | Mesh Size 50micron ,flanged Type | CI | PN10 | 2 |
| 17 | Compensator/Bellows | DN500 | Flanged Type |  | PN10 | 4 |
| 18 | High Temp Ball Valve | DN25 | With Female Thread (Temperature 500°C) |  | PN10 | 5 |
| 19 | Swing type Non Return Valve | DN10 | thread type | CI | PN10 | 2 |
| 20 | Pressure Relief Valve | DN25 | Set Pressure 8bar |  | PN16 | 1 |
| 21 | Y- Type Strainer | DN15 | Mesh Size 0.1 mm | CI | PN16 | 1 |
| 22 | Bilge Ejector | DN80/100 | 45m3/35mwc |  | PN40 | 2 |
| 23 | Pressure Gauge (Dial Type) | 1/4" | (0 to 10)bar | SS |  | 16 |
| 24 | Gauge Cock | 1/4" |  | Brass |  | 35 |
| 25 | Temparature Indicator  | 1/2" | 120deg | SS |  | 10 |
| 26 | Flushing cap with Inner Thread Socket | DN 40 |  | Brass |  | 12 |
| 27 | Sounding cap with chain | DN 40 |  | Brass |  | 6 |
| 28 | Fire Hydrant | DN50 | Flanged,angle Type, storz coupling | Brass | PN10 | 6 |
| 29 | Pressure Reducting Valve | DN25 | 30bar-7bar | Brass | PN40 | 1 |
| 30 | Pressure Relief Valve | DN25 | Set Pressure 8bar |  | PN40 | 1 |
| 31 | swing Check Valve | DN25 |  | CI | PN10 | 1 |
| 32 | Self Closing Sounding cock | DN40 | (with small dia self closing cock) | Brass | PN10 | 9 |
| 33 | Mud box | DN80 | Flangd straight Type | CI | PN10 | 1 |
| 34 | Duplex Fuel Filter | DN40 | Mesh Size100micron ,flanged Type | CI | PN10 | 2 |
| 35 | Y- Type Strainer | DN15 | Mesh Size 0.1 mm | CI | PN10 | 1 |
| 36 | MAGNETIC LEVEL GAUGE |  | Measure Height 1000mm-4800mm |  |  | 10 |
|  Remark |  |
|  Expected Delivery Date |  05/31/2019 |  Max Pack Per Unit |  Tons |